SQ20      An instruction manual
Product characteristics
● High Quality Image HD FULL HD 1080P DV DC
•	Small shape design, portable handheld DV DC

•	High-definition image recording can be performed under low illumination.

•	Video format: 1920 *1080P

•	Mobile Detection Video; 1080P

•	Maximum support for 32G T-flash card

•	Built-in lithium battery for 60 minutes

Operational Guidelines
Charge: This machine has built-in rechargeable lithium batteries. When using this machine for the first time, please charge it first. It can be charged by the following ways:
1. Connect the computer to charge and use USB to connect the computer to charge.
When charging, the red light is always on. The blue light is flashing slowly and the full-charge red and blue light is always on. (After the red and blue light is on, please recharge for about 30 minutes to ensure that the battery is 100% full.)
Be careful:
1 When the battery power is insufficient, the DV red and blue lights flash for 5 seconds and then turn off directly and enter the protective state.
         (Recording file saving and automatic shutdown), please charge the machine at this time.
  2 Turn on without card blue light and turn off automatically after 8 strokes.    
There is no working mode after booting, and it will shut down automatically for 1 minute.
。
  1080P Video Operation:
Press the function button for 5 seconds to turn on the blue lamp for a long time and enter the standby mode. Press the function button once, the blue lamp flashes out three times, and enters 1080P video recording. The lamp does not prompt during the video recording. The continuous video is automatically saved in segments for 5 minutes, and then press the function key for a long time to stop the video recording. The blue lamp will turn on for a long time and return to the standby mode.
1080P Mobile Detection Mode
Long press the function key for 5 seconds to turn on the blue light and enter standby mode. Long press the function key for 3 seconds to turn off the red light for 3 seconds to turn on the mobile detection video mode. When an object is detected moving, the red and blue light simultaneously flashes off the 1080P mobile detection video for 5 minutes, automatically packs and saves, recycles and covers, and no object moves to standby until no electricity or TF card is full. (Press the function key to exit the mobile detection mode with blue light on).
  
  Reset: When the machine crashes, the keys are invalid and can not be used normally, the machine can be reset by pressing the insertion point of the reset hole keys with a pointed object. After reset, the machine can be used normally. Turn off: 
  In the stop (video, mobile detection) mode, it is necessary to shut down, press the function button for about 6 seconds, and turn off all the lights under 5 flashes. When standby mode does not use any function, standby for 1 minute automatically shut down.
  Modify settings at your own time:
When the machine starts, it will automatically create a TIME text document in the TF Kagan directory (as shown in the figure), shut down and connect the computer with the data line. After the movable disk opens the TIME text document, edit the time it needs, such as format (time and seconds of year, month, day) 2017-06-12, 23:59:59 Y, save the text file, boot up and record the video, and the video saved file will show the compiled above. Time of compilation.
Connect the computer:
  In the state of boot, standby and shutdown, the computer can be directly connected. After connecting to the computer, it can be used as a U disk. It is free to copy, clip, delete and format the U disk.
Connect the machine to the computer's USB port. After a few seconds, the computer will pop up the removable disk identification. The red light, blue light and slow flash identification USB device can carry out data transmission.
 Tips:
If the computer is not recognized after connecting to the computer, or if the removable disk still does not pop up after 30 seconds, please reset and re-insert it once.

It is suggested to use TF card reader to read video files directly for playback, while playback of video files stored in the built-in memory of the machine directly through USB connection may cause the playback to be not smooth because of the large amount of data and the transmission can not keep up with it.
Related parameters
project	Relevant parameters	
Video format	AVI	
video coding	M-JPEG	
Video Resolution	1920×1080P   	
Video frame rate	30fps	
Image proportion	16：9	
Vmd	Support	
Battery type	Built-in high-capacity polylithium power	
Battery capacity	240mAh	
Working hours	Sustainable video for 60 minutes	
Charging voltage	DC-5V	
Storage support	Up to 32G TF Cards	
transmission speed	high speed 2.0	
Interface type	Mini 8pin USB	
support system	Windows me/2000/XP/2003/Vista; Mac Os;  Linux;	
Playback software	System-owned or mainstream video and audio playback software	

Use occasion: Please strictly abide by the relevant laws of the country where the product is used, and do not use it for any illegal purposes, otherwise the consequences will be at your own expense.

Working temperature: Please use it at natural temperature, not at temperature that human body can not adapt to.

Work humidity: Please use it under the suitable humidity of human environment. Do not put the product in the humid working environment. This product does not have waterproof function, so as to avoid being caught in water or exposed to rain.