LRS01-V40A Video Lighting CCTV Surge Protection Device DC 5V BNC

LRS01-V40A DC 5V BNC Female Video Lighting Surge Protection Device

CCTV System Single Channel BNC Video Lighting Surge Coax Protector

Features:

Current : max.10KA

Interface : BNC Female

Remote Controlled distance : No

Power Supply : 5V

Impedance : 75Ω;Wire Length : 25cm/ 9.8"

Material : Plastic + aluminum alloy

Easy to install, and can be used for protecting signals of the devices controlled by the low voltage; such as various data transmission circuit, monitoring control circuit, Instrument signal circuit, etc.

Avoid the devices from damages of the lightning overvoltage, electostatic discharge,or induced overvoltage.

Design with the signal ground connection terminal block wire to protect the your devices work well.

Packing List:

1 x Surge Protection Device