Dual-Video Multiplexer Anti-Interference UTP Balun Transceiver for Surveillance System

Surveillance Multiplexer Anti-Interference UTP Transmitter& Receiver for CCTV

Features:

Video anti-interference device:

It can mainly solve the tough anti-interference problems (including elevators, converting stations, electromotor, industrial converter and various high frequency electromagnetic interference)

It can solve various interferential phenomena such as power frequency, common mode and overlapping curve, etc.

Video 1 can transmit the distance of 400 meters to 800 meters (and with function of frequency shift type anti-interference device)

Video 2 can transmit 400 meters (used in conjunction with 640T/R of our company, and the transmission distance can reach 1000 meters)

Video UTP balun transceiver:

Long transmission distance and high image quality

Convenient for wiring and high usage of cable

 Strong anti-interference ability

Packing List:

1 x Transmitter

1 x Receiver

1 x Power cable