# 100PCS UC3843A SOP-8 PWM Controller

# 100PCS Schaltregler Spannungsregler PWM Controller UC3843A SOP-8

**Specification:**

# Product Category: Current Mode PWM ControllersNumber of Outputs: 1Output voltage: 4.9V ~ 5.1VOutput Current: 1000mAuc3843Package: SC-88Operating Supply Voltage: 30VSwitching Frequency: 500 KHzDuty cycle (maximum: 96%)Rise Time: 50nsFall Time: 50nsMaximum operating temperature: + 70 ℃Minimum Operating Temperature: 0 ℃Operating temperature: 0℃to + 70 ℃, -40℃ to + 105℃

# Package: SOIC-8, PDIP-8, SOIC-14



# **Package Included:**

100PCS UC3843A SOP-8