**Title:**

25PCS PWM TL494CN Power Supply Controllers DIP-16

25PCS TL494CN DIP-16 PWM Control Integrated Circuit

**Description:**

Product Category: Voltage Mode PWM Controllers

Number of Outputs: Dual

Output Voltage: 40 V (Max)

Output Current: 200 mA (Max)

Switching Frequency: 300 KHz

Synchronous Pin: No

Duty Cycle (Max): 45 % (Typ)

Rise Time: 100 ns

Fall Time: 40 ns

Maximum Operating Temperature: 70 ℃

Minimum Operating Temperature: 0 ℃

Package: DIP-16

**Package Included:**

25PCS PWM TL494CN Power Supply Controllers