**Title:**

25PCS CD4511BE 7 Segment Decoder Driver C-MOS Integrated Circuit DIP-16

25PCS CD4511BE DIP-16 7 Segment Decoder Driver C-MOS IC For Electronic Product

**Description:**

Decoder /Driver IC

BCD to 7 segment LED display

Logic Case Style: DIP

Logic Type: BCD to 7 Segment Decoder / Driver / Latch

No. of Outputs: 7

No. of Pins: 16

Operating Temperature Max: 125°C

Operating Temperature Min: -55°C

Supply Voltage Max: 18V

Supply Voltage Min: 3V

**Package Included:**

25PCS CD4511BE 7 Segment Decoder Driver